,Connection Size##pipe_size##millimeters,Maximum Working Pressure##piping_pressure##pounds_force_per_square_inch,Minimum Operating Temperature##hvac_temperature##fahrenheit,Maximum Operating Temperature##hvac_temperature##fahrenheit,Minimum Flow Rate Value##number##general,Maximum Flow Rate Value##number##general,Unit Weight##force##kilograms_force,Connection Type##other##,Flow Configuration##other##,Description##other##,Model##other##,URL##other##,Product Page URL##other##,Body Material##other##,CV (liters per second)##other##,K Coefficient##number##general,Connection to Connection##length##inches,Cover Upper Flange Diameter##length##inches,Connection Axis to Valve Top##length##inches,Connection Axis to Valve Bottom##length##inches,Grooved Outside Diameter##length##inches,Grooved Diameter##length##inches,Grooved End Length##length##inches,Grooved Length##length##inches,Side Port Outside Diameter##length##inches,Pipe Plug Circumscribe Length##length##inches,X Pilot System Offset##length##inches,Y Pilot System Offset##length##inches,Z Pilot System Offset##length##inches
81-12_Ductile_Iron_40mm,40,400,-40,180,0,38,6.80388555,Grooved,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,2.0,5.9,8.5,5.62,4.75,2.0,1.9,1.775,0.63,0.313,0.375,0.25,11,9,9
81-12_Ductile_Iron_50mm,50,400,-40,180,0,64,15.87573295,Grooved,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,3.4,5.6,9.0,6.62,5.75,2.5,2.375,2.25,0.63,0.313,0.375,0.5,13,9,9
81-12_Ductile_Iron_65mm,65,400,-40,180,0,90,22.6796185,Grooved,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,5.4,4.6,11.0,8.0,6.88,2.88,2.875,2.72,0.63,0.313,0.5,0.5,14,10,10
81-12_Ductile_Iron_80mm,80,400,-40,180,0,140,31.7514659,Grooved,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,7.3,6.0,12.5,9.12,7.25,3.12,3.5,3.344,0.63,0.313,0.5,0.5,15,11,11
81-12_Ductile_Iron_100mm,100,400,-40,180,0,240,63.5029318,Grooved,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,13.0,5.9,15.0,11.5,9.31,4.25,4.5,4.344,0.63,0.375,0.75,0.75,17,12,12
