,Connection Size##pipe_size##millimeters,Maximum Working Pressure##piping_pressure##pounds_force_per_square_inch,Minimum Operating Temperature##hvac_temperature##fahrenheit,Maximum Operating Temperature##hvac_temperature##fahrenheit,Minimum Flow Rate Value##number##general,Maximum Flow Rate Value##number##general,Unit Weight##force##kilograms_force,Connection Type##other##,Flow Configuration##other##,Description##other##,Model##other##,URL##other##,Product Page URL##other##,Body Material##other##,Standards##other##,CV (liters per second)##other##,K Coefficient##number##general,Connection to Connection##length##inches,Cover Upper Flange Diameter##length##inches,Connection Axis to Valve Top##length##inches,Flange Outside Radius##length##inches,Side Port Outside Diameter##length##inches,Pipe Plug Circumscribe Length##length##inches,X Pilot System Offset##length##inches,Y Pilot System Offset##length##inches,Z Pilot System Offset##length##inches
81-12_Ductile_Iron_C150_40mm,40,250,-40,180,0,125,6.80388555,Flanged,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,ASTM A536 B16.42,2.0,5.9,8.5,5.62,5.5,2.5,0.375,0.25,11,9,9
81-12_Ductile_Iron_C150_50mm,50,250,-40,180,0,210,15.87573295,Flanged,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,ASTM A536 B16.42,3.4,5.6,9.38,6.62,6.5,3.0,0.375,0.5,13,9,9
81-12_Ductile_Iron_C150_65mm,65,250,-40,180,0,300,22.6796185,Flanged,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,ASTM A536 B16.42,5.4,4.6,11.0,8.0,7.56,3.5,0.5,0.5,14,10,10
81-12_Ductile_Iron_C150_80mm,80,250,-40,180,0,460,31.7514659,Flanged,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,ASTM A536 B16.42,7.3,6.0,12.0,9.12,8.19,3.75,0.5,0.5,15,11,11
81-12_Ductile_Iron_C150_100mm,100,250,-40,180,0,800,63.5029318,Flanged,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,ASTM A536 B16.42,13.0,5.9,15.0,11.5,10.62,4.5,0.75,0.75,17,12,12
81-12_Ductile_Iron_C300_40mm,40,400,-40,180,0,125,6.80388555,Flanged,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,ASTM A536 B16.42,2.0,5.9,9.0,5.62,5.5,3.06,0.375,0.25,11,9,9
81-12_Ductile_Iron_C300_50mm,50,400,-40,180,0,210,15.87573295,Flanged,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,ASTM A536 B16.42,3.4,5.6,10.0,6.62,6.5,3.25,0.375,0.5,13,9,9
81-12_Ductile_Iron_C300_65mm,65,400,-40,180,0,300,22.6796185,Flanged,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,ASTM A536 B16.42,5.4,4.6,11.62,8.0,7.56,3.75,0.5,0.5,14,10,10
81-12_Ductile_Iron_C300_80mm,80,400,-40,180,0,460,31.7514659,Flanged,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,ASTM A536 B16.42,7.3,6.0,13.25,9.12,8.19,4.13,0.5,0.5,15,11,11
81-12_Ductile_Iron_C300_100mm,100,400,-40,180,0,800,63.5029318,Flanged,In/Out,Check Valve,81-12,https://www.cla-val.com/,https://www.cla-val.com/waterworks/check-valves/81-12,Metal - Cla-Val - Ductile Iron - Blue,ASTM A536 B16.42,13.0,5.9,15.62,11.5,10.62,5.0,0.75,0.75,17,12,12
